INSTALLATION NOTES FOR ICE.TCP WITH NOVELL'S ODI STACK

This release note describes the installation procedure using
ICE.TCP with Novell's ODI protocol stack.

The files included, ODIPKT3.COM, ODIPKT2.COM, and ODIPKT.DOC are copyright
by Daniel D. Lanciani.  Although James River Group includes this software
with ICE.TCP, we do not guarantee its performance.  This software is
distributed as a service to our customers.
 

INSTALLATION NOTES 
 
The following files are found in the \ODI directory of the
ICE.TCP distribution disk. 
 
READODI.ME          This Document 
 
ODIPKT2.COM         The ODI shim for use with ICE.TCP

ODIPKT3.COM         More recent version of same.  May work with PCMCIA.

ODIPKT.DOC          The original installation instructions        
                    from the author of ODIPKT.COM

AUTOEXEC.ODI        An example AUTOEXEC.BAT for use with ICE.TCP 

CONFIG.ODI          An example CONFIG.SYS for use with ICE.TCP    

NET.ICE             An example NET.CFG file for ethernet
                    (if you are using ARCnet or Token Ring
                    please see the release notes included with
                    ICE.TCP)

First, follow the instructions in the ICE.TCP manual on page 3
titled "DOS INSTALLATION".  Do not forget to run custom on
NETDEV.SYS as described in the ICE.TCP manual.
 
You will not need to use any of the network adapter drivers
(packet drivers) that we supply.  The ODIPKT2.COM will take the
place of the packet driver.  You should use the ODI network
adapter driver that network card manufacturer supplies as
instructed in the ODI manual.  If you have any questions on what
driver to use, consult your network adapter instructions under
"ODI" support. 
 
You should now have a directory (C:\ICETCP) where all of your
ICE.TCP files are stored.  You should also have a DOS environment
variable set; called "ICETCP" set to the directory where your
ICE.TCP files reside. 
 
Next, modify your CONFIG.SYS file.  A sample CONFIG.ICE file is
included with this distribution.  The part of the CONFIG.ICE that
pertains to this installation is:
 
device=[drive][path]NETDEV.SYS 
 
Next alter your AUTOEXEC.BAT file to include the ODIPKT2.COM
driver AFTER you have loaded all the other ODI drivers (LSL, LAN
ADAPTER DRIVER, IPXODI, etc).  Again, a sample AUTOEXEC.ICE file
is included.
 
All of the examples in the included sample files assume that your
protocol stack configuration files are located in a C:\ODI
directory, and that your ICE.TCP files are in a directory named
"C:\ICETCP". 
 
Once you have modified and loaded the protocol stack, you should
be ready to run ICE.TCP.